# COMMISSION ACTION MATRIXSTRUCTURAL DESIGN/LATERAL FORCES (SDLF) CODE ADVISORY COMMITTEE – JULY 16-17, 2024

## 2025 CALIFORNIA ADMINISTRATIVE CODE, TITLE 24, PART 1AGENCY: Office of Statewide Hospital Planning and Development, OSHPD 03/24

### LEGEND:

**CAC Actions:** Approve, Disapprove, Approve as Amended, Further Study Required

**Agency Responses:** Accept, Disagree, Withdraw

**CBSC Actions:** Approve, Disapprove, Approve as Amended, Further Study Required

**Matrix Paper Color** (for commission action only): GREEN = uncontested items, YELLOW = challenged items, SALMON = withdrawn, no action required

If using assistive technology, please adjust your settings to recognize underline, strikeout and ellipsis.

* Existing California amendments appear upright
* Amended or new California amendments appear underlined
* Repealed California language appears ~~upright and in strikeout~~
* Ellipses (…) indicate existing text remains unchanged

### ITEM 1CHAPTER 6 SEISMIC EVALUATION PROCEDURES FOR HOSPITAL BUILDINGS, ARTICLE 1 DEFINITIONS AND REQUIREMENTS

Amend Chapter 6 subtitle and sections as listed below.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **OSHPD 03/24ITEM 1** | **Code Section** | **CACAction** | **Agency Response** | **Public Comments** | **Annotations** | **CBSCAction** |
| **1-1** | **ADMINISTRATIVE REGULATIONS FOR THE OFFICE OF STATEWIDE ~~HEALTH~~ HOSPITAL PLANNING AND DEVELOPMENT (OSHPD)** |  |  |  | Amend Health to Hospital. |  |
| **1-2** | **1.2 Definitions.****~~ADMINISTRATIVE EXTENSION~~** |  |  |  | Repeal entire definition. |  |
| **1-3** | **~~CRITICAL COMMUNITY PROVIDER~~** |  |  |  | Repeal entire definition. |  |
| **1-4** | **DAMAGE CONTROL STRUCTURAL PERFORMANCE CATEGORY** |  |  |  | Change code section references and make editorial amendments. |  |
| **1-5** | **GENERAL ACUTE CARE HOSPITAL** |  |  |  | Editorial amendments. |  |
| **1-6** | **PROBABILITY OF COLLAPSE** |  |  |  | Change code section reference. |  |
| **1-7** | **STRUCTURAL PERFORMANCE CATEGORY SPC-4D** |  |  |  | Change code section references and make editorial amendments. |  |
| **1-8** | **1.3 Seismic evaluation.** |  |  |  | An editorial revision to the Exception for proper reference to code sections. Repeal language with conflicting regulations. |  |
| **1-9** | **1.4 Compliance plans.** |  |  |  | Editorial amendments. |  |
| **1-10** | **1.4.4.4 Compliance plan schedule.** |  |  |  | Correct organization name for California Department of Public Health (CDPH). |  |
| **1-11** | **1.4.5 Compliance plan update/change notification.** |  |  |  | Deadline established for submittal of revised compliance plans. |  |
| **1-12** | **1.4.5.1 Change in seismic performance category.** |  |  |  | Editorial amendments. |  |
| **1-13** | **1.4.5.1.3** |  |  |  | An editorial revision for proper reference to code sections Repeal language with conflicting regulations. |  |
| **1-14** | **1.5.2 Delay in compliance. #1 Requirements for NPC.** |  |  |  | Repeal reference to “Seismic Design Category D”; replace “January” with “March” in subsections 1.2, 1.3 and 1.4; Add exception to subsection 1.2. for buildings that have been removed from acute care (or plan to be removed by 2030); clarify NPC rating level and specify compliance categories in subsection 1.4. |  |
| **1-15** | **1.5.2 Delay in compliance. #2 Requirements for SPC.** |  |  |  | Repeal subsection 1 through 1.8 (per AB 2190) and renumber subsequent subsections accordingly.  |  |

### ITEM 2CHAPTER 6, ARTICLE 11 EVALUATION OF CRITICAL NONSTRUCTURAL COMPONENTS AND SYSTEMS

Amend sections as listed below.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **OSHPD 03/24ITEM 2** | **Code Section** | **CACAction** | **Agency Response** | **Public Comments** | **Annotations** | **CBSCAction** |
| **2-1** | **11.2.3 Evaluation procedures for NPC 4 and NPC 4D.**  |  |  |  | Amend “Level 1” to “NPC 3” Areas and clarify requirements for showing utilities on the plans. |  |
| **2-2** | **11.3.1 Anchors used in the seismic bracing of pipes, ducts or conduit.**  |  |  |  | Repeal torque testing requirements for bolts with no tension. |  |
| **2-3** | **11.3.2** **Anchors used in the attachment of equipment and other components.** **Subsection 1.** |  |  |  | Repeal torque testing requirements for bolts with no tension. |  |
| **2-4** | **~~11.3.5 Allowable shear loads.~~** |  |  |  | Section repealed; requirements addressed by new Section 11.4. |  |
| **2-5** | **11.4 Capacity of existing mechanical anchors:** |  |  |  | New section comprised of repealed Section 11.3.5 with clarifications. |  |

### ITEMS 3 THROUGH 8 ARE HEARD BY THE HEALTH FACILITIES (HF) CODE ADVISORY COMMITTEE ON JULY 30, 2024. CHAPTER 7 SAFETY STANDARDS FOR HEALTH FACILITIES